{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["台式机"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"台式机","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[[1,0,1,8],[46,2,46,8]],"flags":["formulas_cached_only"]}
["附件1"]
["中央国家机关台式计算机批量集中采购配置标准（2025版）"]
["序号","指 标 项","配置1","配置2","配置3","配置4","配置5","配置6","配置7（采购单位选此项配置应符合相关管理要求）"]
[1,"预算上限（人民币 元）",5000,5000,5000,5000,5000,5000,5000]
[2,"CPU品牌","龙芯","飞腾","兆芯","华为鲲鹏","海光","申威","Intel/AMD"]
[3,"CPU型号","≥3A6000","≥腾锐D3000","≥KX-7000","≥麒麟9000C","≥C86-3G","≥SW-WY831","≥I5-12500或≥Ryzen5 5600G"]
[4,"CPU主频（基准时钟频率，GHz）","≥2.5","≥2.5","≥3.6","≥2.3","≥2.8","≥2.5","≥2.1"]
[5,"CPU物理核数","≥4","≥8","≥8","≥8","≥8","≥8","≥6"]
[6,"主板芯片组型号","/","/","/","/","/","/","≥Q670或Pro565"]
[7,"显示屏尺寸（英寸）","≥23.8","≥23.8","≥23.8","≥23.8","≥23.8","≥23.8","≥23.8"]
[8,"显示屏分辨率","≥1920*1080","≥1920*1080","≥1920*1080","≥1920*1080","≥1920*1080","≥1920*1080","≥1920*1080"]
[9,"显示屏色准","最大△E ≤4","最大△E ≤4","最大△E ≤4","最大△E ≤4","最大△E ≤4","最大△E ≤4","最大△E ≤4"]
[10,"显示屏响应时间（ms）","≤8","≤8","≤8","≤8","≤8","≤8","≤8"]
[11,"显示屏可视角度","≥170°/160°","≥170°/160°","≥170°/160°","≥170°/160°","≥170°/160°","≥170°/160°","≥170°/160°"]
[12,"显示屏材质","VA/IPS","VA/IPS","VA/IPS","VA/IPS","VA/IPS","VA/IPS","VA/IPS"]
[13,"显示屏屏幕比例","16:9","16:9","16:9","16:9","16:9","16:9","16:9"]
[14,"内存配置容量","≥8GB","≥8GB","≥8GB","≥8GB","≥8GB","≥8GB","≥16GB"]
[15,"内存读写速率","≥3200MT/s","≥3200MT/s","≥3200MT/s","≥3200MT/s","≥3200MT/s","≥3200MT/s","≥3200MT/s"]
[16,"内存扩展接口 (板载内存不涉及)","≥2","≥2","≥2","≥2","≥2","≥2","≥2"]
[17,"硬盘类型","机械硬盘+固态硬盘","机械硬盘+固态硬盘","机械硬盘+固态硬盘","机械硬盘+固态硬盘","机械硬盘+固态硬盘","机械硬盘+固态硬盘","机械硬盘+固态硬盘"]
[18,"机械硬盘接口方式","SATAIII","SATAIII","SATAIII","SATAIII","SATAIII","SATAIII","SATAIII"]
[19,"机械硬盘转速（RPM）","≥5400","≥5400","≥5400","≥5400","≥5400","≥5400","≥5400"]
[20,"机械硬盘总容量","≥1TB","≥1TB","≥1TB","≥1TB","≥1TB","≥1TB","≥1TB"]
[21,"固态存储容量","≥256GB","≥256GB","≥256GB","≥256GB","≥256GB","≥256GB","≥512GB"]
[22,"显卡类型","独立显卡","独立显卡","独立显卡","集成显卡","独立显卡","独立显卡","集成显卡"]
[23,"独立显卡显存容量","≥2GB","≥2GB","≥2GB","/","≥2GB","≥2GB","/"]
[24,"独立显卡显存位宽（bit）","≥32","≥64","≥64","/","≥64","≥64","/"]
[25,"独立显卡显存类型","DDR4/LPDDR4/GDDR5/GDDR6","DDR4/LPDDR4/GDDR5/GDDR6","DDR4/LPDDR4/GDDR5/GDDR6","/","DDR4/LPDDR4/GDDR5/GDDR6","DDR4/LPDDR4/GDDR5/GDDR6","/"]
[26,"预装正式版操作系统（最新版且永久授权）","麒麟/统信UOS/中科方德/其他符合安全可靠测评要求的操作系统","麒麟/统信UOS/中科方德/其他符合安全可靠测评要求的操作系统","麒麟/统信UOS/中科方德/其他符合安全可靠测评要求的操作系统","麒麟/统信UOS/中科方德/其他符合安全可靠测评要求的操作系统","麒麟/统信UOS/中科方德/其他符合安全可靠测评要求的操作系统","麒麟/统信UOS/中科方德/其他符合安全可靠测评要求的操作系统","Windows10神州网信版"]
[27,"是否有刻录光驱","是","是","是","是","是","是","是"]
[28,"内置集成声卡","是","是","是","是","是","是","是"]
[29,"有线网卡数量","≥1","≥1","≥1","≥1","≥1","≥1","≥1"]
[30,"USB接口数量","≥8个，其中USB3.0及以上标准接口≥4个","≥8个，其中USB3.0及以上标准接口≥4个","≥8个，其中USB3.0及以上标准接口≥4个","≥8个，其中USB3.0及以上标准接口≥4个","≥8个，其中USB3.0及以上标准接口≥4个","≥8个，其中USB3.0及以上标准接口≥4个","≥8个，其中USB3.0及以上标准接口≥4个"]
[31,"HDMI接口","≥1","≥1","≥1","≥1","≥1","≥1","≥1"]
[32,"VGA接口","≥1","≥1","≥1","≥1","≥1","≥1","≥1"]
[33,"网络接口","≥1","≥1","≥1","≥1","≥1","≥1","≥1"]
[34,"显示器和机身颜色","黑色/灰色/银色等商务色系均可","黑色/灰色/银色等商务色系均可","黑色/灰色/银色等商务色系均可","黑色/灰色/银色等商务色系均可","黑色/灰色/银色等商务色系均可","黑色/灰色/银色等商务色系均可","黑色/灰色/银色等商务色系均可"]
[35,"鼠标","有线（USB)","有线（USB)","有线（USB)","有线（USB)","有线（USB)","有线（USB)","有线（USB)"]
[36,"键盘","有线（USB)","有线（USB)","有线（USB)","有线（USB)","有线（USB)","有线（USB)","有线（USB)"]
[37,"键盘按键数目","104键","104键","104键","104键","104键","104键","104键"]
[38,"有线键盘连接线","≥1.5米","≥1.5米","≥1.5米","≥1.5米","≥1.5米","≥1.5米","≥1.5米"]
[39,"关键部件安全要求","CPU和操作系统等关键部件应当符合安全可靠测评要求","CPU和操作系统等关键部件应当符合安全可靠测评要求","CPU和操作系统等关键部件应当符合安全可靠测评要求","CPU和操作系统等关键部件应当符合安全可靠测评要求","CPU和操作系统等关键部件应当符合安全可靠测评要求","CPU和操作系统等关键部件应当符合安全可靠测评要求","/"]
[40,"其他要求","财政部《台式计算机政府采购需求标准》中规定的其他*内容","财政部《台式计算机政府采购需求标准》中规定的其他*内容","财政部《台式计算机政府采购需求标准》中规定的其他*内容","财政部《台式计算机政府采购需求标准》中规定的其他*内容","财政部《台式计算机政府采购需求标准》中规定的其他*内容","财政部《台式计算机政府采购需求标准》中规定的其他*内容","财政部《台式计算机政府采购需求标准》中规定的除安全可靠测评要求外的其他*内容"]
[41,"是否具有节能产品认证证书（有效期内）","是","是","是","是","是","是","是"]
[42,"是否为进口产品","否","否","否","否","否","否","否"]
[43,"整机质量服务要求","免费服务周期（含换件和维修）≥3年","免费服务周期（含换件和维修）≥3年","免费服务周期（含换件和维修）≥3年","免费服务周期（含换件和维修）≥3年","免费服务周期（含换件和维修）≥3年","免费服务周期（含换件和维修）≥3年","免费服务周期（含换件和维修）≥3年"]
[44,"服务标准","a)供应商提供电话、电子邮件、远程连接等多种形式服务；\nb)供应商提供同城4小时、异地12小时技术响应服务，2个工作日解决问题，对于未能解决的问题和故障应提供可行的升级方案，并提供周转设备或更换设备；\nc)建立全国技术服务体系和服务团体，符合专业服务体系标准要求，提供原厂中文服务；\nd)服务周期内提供产品的维修、换件和升级服务；\ne)免费送货到采购人指定的地点。"]